<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="24.13" y2="0" width="0" layer="20"/>
<wire x1="24.13" y1="0" x2="24.13" y2="16.51" width="0" layer="20"/>
<wire x1="24.13" y1="16.51" x2="1.27" y2="16.51" width="0" layer="20"/>
<wire x1="1.27" y1="16.51" x2="1.27" y2="0" width="0" layer="20"/>
<text>1-Wire Term/Pull-up</text>
<text>Tempberry Pi 
Sensor System</text>
</plain>
<libraries>
<library name="NA-lib">
<packages>
<package name="RJ-12-SHORT">
</package>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="NA-lib" package="RJ-12-SHORT" value="PULSE_E5566-Q0LK22-L">
<attribute name="NAME"/>
</element>
<element name="J2" library="NA-lib" package="RJ-12-SHORT" value="PULSE_E5566-Q0LK22-L"/>
<element name="R1" library="NA-lib" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="NA-lib" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="1WIRE_DATA">
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
