<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="77.216" y2="0" width="0" layer="20"/>
<wire x1="77.216" y1="15.24" x2="0" y2="15.24" width="0" layer="20"/>
<wire x1="0" y1="15.24" x2="0" y2="0" width="0" layer="20"/>
<wire x1="77.216" y1="15.24" x2="95.936" y2="7.62" width="0" layer="20" curve="-38.905931"/>
<wire x1="77.216" y1="0" x2="95.936" y2="7.62" width="0" layer="20" curve="38.905931"/>
<text>30</text>
<text>25</text>
<text>20</text>
<text>15</text>
<text>10</text>
<text>5</text>
<text>0</text>
<text>25</text>
<text>20</text>
<text>15</text>
<text>10</text>
<text>5</text>
<text>0</text>
<text>Soil Sensor [1-zone] r2</text>
<text>Copyright OSU CGRB,
Tyler and Jaiswal Labs.</text>
<text>Humidity measured 
63 mm above soil</text>
<text>mm</text>
<text>mm</text>
<text>Soil  Level</text>
<text>Soil  Level</text>
<text>Designed by Nick Ames</text>
</plain>
<libraries>
<library name="NA-lib">
<packages>
<package name="QFN-32-0.5-EP">
</package>
<package name="RJ-12-SHORT">
</package>
<package name="WLCSP-6">
</package>
<package name="DFN3030-6">
</package>
<package name="SOT-323-3">
</package>
<package name="0402">
</package>
<package name="0603-RES">
</package>
<package name="TXC-8Y">
</package>
<package name="SOD-323">
</package>
<package name="0603-CAP-POL">
</package>
<package name="DUAL_LED_1206">
</package>
<package name="HMD8">
</package>
<package name="SOIL_MOISTURE_SENSOR_V1">
</package>
<package name="LSCSP-8">
</package>
<package name="UDFN-4">
</package>
<package name="804-RES-4ARRAY">
</package>
<package name="CKCM25">
</package>
<package name="CKCA43">
</package>
<package name="TESTPOINT-POGO-HOLE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="NA-lib" package="QFN-32-0.5-EP" value="ATMEGA88MU">
<attribute name="NAME"/>
</element>
<element name="J1" library="NA-lib" package="RJ-12-SHORT" value="PULSE_E5566-Q0LK22-L&quot;">
<attribute name="NAME"/>
</element>
<element name="J2" library="NA-lib" package="RJ-12-SHORT" value="PULSE_E5566-Q0LK22-L&quot;">
<attribute name="NAME"/>
</element>
<element name="U4" library="NA-lib" package="WLCSP-6" value="TI_TMP108">
<attribute name="NAME"/>
</element>
<element name="U3" library="NA-lib" package="DFN3030-6" value="SI7006">
<attribute name="NAME"/>
</element>
<element name="F1" library="NA-lib" package="0603-RES" value="100mA PTC">
<attribute name="NAME"/>
</element>
<element name="X1" library="NA-lib" package="TXC-8Y" value="16Mhz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="NA-lib" package="SOT-323-3" value="12V">
<attribute name="NAME"/>
</element>
<element name="D1" library="NA-lib" package="SOD-323" value="5.6V">
<attribute name="NAME"/>
</element>
<element name="C3" library="NA-lib" package="0402" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="NA-lib" package="0603-CAP-POL" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="D4" library="NA-lib" package="DUAL_LED_1206" value="LTST-S326KGJRKT">
<attribute name="NAME"/>
</element>
<element name="D5" library="NA-lib" package="HMD8" value="RB521ZS8A30TE61">
<attribute name="NAME"/>
</element>
<element name="C6" library="NA-lib" package="SOIL_MOISTURE_SENSOR_V1" value=""/>
<element name="U2" library="NA-lib" package="LSCSP-8" value="ADM4850ACPZ">
<attribute name="NAME"/>
</element>
<element name="U5" library="NA-lib" package="UDFN-4" value="TLV70733">
<attribute name="NAME"/>
</element>
<element name="R4" library="NA-lib" package="804-RES-4ARRAY" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="NA-lib" package="CKCM25" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="NA-lib" package="CKCA43" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="NA-lib" package="CKCA43" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="NA-lib" package="0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="NA-lib" package="0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="NA-lib" package="0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="NA-lib" package="TESTPOINT-POGO-HOLE" value="3V3"/>
<element name="TP4" library="NA-lib" package="TESTPOINT-POGO-HOLE" value="!RST"/>
<element name="TP5" library="NA-lib" package="TESTPOINT-POGO-HOLE" value="MOSI"/>
<element name="TP6" library="NA-lib" package="TESTPOINT-POGO-HOLE" value="SCK"/>
<element name="TP7" library="NA-lib" package="TESTPOINT-POGO-HOLE" value="MISO"/>
</elements>
<signals>
<signal name="J_MISO">
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="A">
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="U2" pad="6"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="B">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="J_RESET">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="F1" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="8"/>
<contactref element="U5" pad="4"/>
<contactref element="U5" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="C2" pad="+"/>
<contactref element="C1" pad="C1"/>
<contactref element="C1" pad="D1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="7"/>
<contactref element="X1" pad="X1"/>
<contactref element="C5" pad="B1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="8"/>
<contactref element="X1" pad="X2"/>
<contactref element="C5" pad="A1"/>
</signal>
<signal name="RS-485R">
<contactref element="U1" pad="30"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="RS-485D">
<contactref element="U1" pad="31"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="RS-485_D/!R">
<contactref element="U1" pad="32"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="PAD"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="D2" pad="3"/>
<contactref element="U4" pad="A2"/>
<contactref element="U3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="PAD"/>
<contactref element="U5" pad="2"/>
<contactref element="U5" pad="PAD"/>
<contactref element="D1" pad="A"/>
<contactref element="C2" pad="-"/>
<contactref element="C5" pad="A2"/>
<contactref element="C5" pad="B2"/>
<contactref element="C4" pad="A2"/>
<contactref element="C4" pad="B2"/>
<contactref element="C4" pad="C2"/>
<contactref element="C4" pad="D2"/>
<contactref element="C1" pad="C2"/>
<contactref element="C1" pad="D2"/>
<contactref element="C1" pad="A2"/>
<contactref element="C1" pad="B2"/>
<contactref element="X1" pad="GND"/>
</signal>
<signal name="SDA">
<contactref element="U4" pad="C2"/>
<contactref element="U1" pad="27"/>
<contactref element="U3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U4" pad="B2"/>
<contactref element="U1" pad="28"/>
<contactref element="U3" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="LED_A">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="LED_A_POSTRES">
<contactref element="D4" pad="ANODE"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="LED_G_C">
<contactref element="D4" pad="C_GREEN"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="LED_R_C">
<contactref element="D4" pad="C_RED"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="M_DRIVE">
<contactref element="U1" pad="12"/>
<contactref element="R4" pad="D2"/>
<contactref element="R4" pad="C2"/>
<contactref element="R4" pad="B2"/>
<contactref element="R4" pad="A2"/>
</signal>
<signal name="M_ZONE0">
<contactref element="D5" pad="C1"/>
<contactref element="C4" pad="A1"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="M_ZONE1">
<contactref element="U1" pad="23"/>
<contactref element="D5" pad="C2"/>
<contactref element="C4" pad="B1"/>
</signal>
<signal name="M_ZONE2">
<contactref element="D5" pad="C3"/>
<contactref element="C4" pad="C1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="M_ZONE3">
<contactref element="D5" pad="C4"/>
<contactref element="C4" pad="D1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="CZ0">
<contactref element="C6" pad="1"/>
<contactref element="D5" pad="A1"/>
<contactref element="R4" pad="D1"/>
</signal>
<signal name="CZ1">
<contactref element="D5" pad="A2"/>
<contactref element="R4" pad="C1"/>
</signal>
<signal name="CZ2">
<contactref element="D5" pad="A3"/>
<contactref element="R4" pad="B1"/>
</signal>
<signal name="CZ3">
<contactref element="D5" pad="A4"/>
<contactref element="R4" pad="A1"/>
</signal>
<signal name="3V3">
<contactref element="U3" pad="5"/>
<contactref element="U4" pad="A1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="A1"/>
<contactref element="C1" pad="B1"/>
<contactref element="U5" pad="1"/>
<contactref element="U4" pad="B1"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="TP2" pad="T"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="14"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="TP7" pad="T"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="TP6" pad="T"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="TP5" pad="T"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="TP4" pad="T"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
