<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>put this part to soil</text>
<text>Plant watering alarm v.2.4</text>
<text>http://wemakethings.net/chirp</text>
<text>ISP</text>
<text>CERN OHL</text>
<text>v.1.1</text>
<text>chirp!</text>
<wire x1="145.415" y1="9.271" x2="129.54" y2="17.272" width="1.524" layer="46" curve="42"/>
<wire x1="4.318" y1="15.494" x2="4.318" y2="2.286" width="1.524" layer="46"/>
<wire x1="6.096" y1="0.508" x2="73.66" y2="0.508" width="1.524" layer="46"/>
<wire x1="76.2" y1="0.508" x2="127" y2="0.508" width="1.524" layer="46"/>
<wire x1="145.415" y1="9.271" x2="129.54" y2="17.272" width="1.27" layer="46" curve="41"/>
<wire x1="145.669" y1="8.763" x2="129.54" y2="0.508" width="1.524" layer="46" curve="-42"/>
<wire x1="6.096" y1="17.272" x2="73.66" y2="17.272" width="1.524" layer="46"/>
<wire x1="76.2" y1="17.272" x2="127" y2="17.272" width="1.524" layer="46"/>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>D1</text>
<text>D2</text>
<text>IC1</text>
<text>JP1</text>
<text>LED1</text>
<text>Q1</text>
<text>Q1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>SP1</text>
<text>put this part to soil</text>
<text>Plant watering alarm v.2.4</text>
<text>http://wemakethings.net/chirp</text>
<text>ISP</text>
<text>CERN OHL</text>
<text>v.1.1</text>
<text>chirp!</text>
<wire x1="145.415" y1="29.591" x2="129.54" y2="37.592" width="1.524" layer="46" curve="42"/>
<wire x1="4.318" y1="35.814" x2="4.318" y2="22.606" width="1.524" layer="46"/>
<wire x1="6.096" y1="20.828" x2="73.66" y2="20.828" width="1.524" layer="46"/>
<wire x1="76.2" y1="20.828" x2="127" y2="20.828" width="1.524" layer="46"/>
<wire x1="145.415" y1="29.591" x2="129.54" y2="37.592" width="1.27" layer="46" curve="41"/>
<wire x1="145.669" y1="29.083" x2="129.54" y2="20.828" width="1.524" layer="46" curve="-42"/>
<wire x1="6.096" y1="37.592" x2="73.66" y2="37.592" width="1.524" layer="46"/>
<wire x1="76.2" y1="37.592" x2="127" y2="37.592" width="1.524" layer="46"/>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>D1</text>
<text>D2</text>
<text>IC1</text>
<text>JP1</text>
<text>LED1</text>
<text>Q1</text>
<text>Q1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>SP1</text>
<text>put this part to soil</text>
<text>Plant watering alarm v.2.4</text>
<text>http://wemakethings.net/chirp</text>
<text>ISP</text>
<text>CERN OHL</text>
<text>v.1.1</text>
<text>chirp!</text>
<wire x1="145.415" y1="49.911" x2="129.54" y2="57.912" width="1.524" layer="46" curve="42"/>
<wire x1="4.318" y1="56.134" x2="4.318" y2="42.926" width="1.524" layer="46"/>
<wire x1="6.096" y1="41.148" x2="73.66" y2="41.148" width="1.524" layer="46"/>
<wire x1="76.2" y1="41.148" x2="127" y2="41.148" width="1.524" layer="46"/>
<wire x1="145.415" y1="49.911" x2="129.54" y2="57.912" width="1.27" layer="46" curve="41"/>
<wire x1="145.669" y1="49.403" x2="129.54" y2="41.148" width="1.524" layer="46" curve="-42"/>
<wire x1="6.096" y1="57.912" x2="73.66" y2="57.912" width="1.524" layer="46"/>
<wire x1="76.2" y1="57.912" x2="127" y2="57.912" width="1.524" layer="46"/>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>D1</text>
<text>D2</text>
<text>IC1</text>
<text>JP1</text>
<text>LED1</text>
<text>Q1</text>
<text>Q1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>SP1</text>
<text>put this part to soil</text>
<text>Plant watering alarm v.2.4</text>
<text>http://wemakethings.net/chirp</text>
<text>ISP</text>
<text>CERN OHL</text>
<text>v.1.1</text>
<text>chirp!</text>
<wire x1="145.415" y1="70.231" x2="129.54" y2="78.232" width="1.524" layer="46" curve="42"/>
<wire x1="4.318" y1="76.454" x2="4.318" y2="63.246" width="1.524" layer="46"/>
<wire x1="6.096" y1="61.468" x2="73.66" y2="61.468" width="1.524" layer="46"/>
<wire x1="76.2" y1="61.468" x2="127" y2="61.468" width="1.524" layer="46"/>
<wire x1="145.415" y1="70.231" x2="129.54" y2="78.232" width="1.27" layer="46" curve="41"/>
<wire x1="145.669" y1="69.723" x2="129.54" y2="61.468" width="1.524" layer="46" curve="-42"/>
<wire x1="6.096" y1="78.232" x2="73.66" y2="78.232" width="1.524" layer="46"/>
<wire x1="76.2" y1="78.232" x2="127" y2="78.232" width="1.524" layer="46"/>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>D1</text>
<text>D2</text>
<text>IC1</text>
<text>JP1</text>
<text>LED1</text>
<text>Q1</text>
<text>Q1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>SP1</text>
<wire x1="-2.54" y1="-3.81" x2="-2.54" y2="82.55" width="0" layer="20"/>
<wire x1="-2.54" y1="82.55" x2="149.86" y2="82.55" width="0" layer="20"/>
<wire x1="149.86" y1="82.55" x2="149.86" y2="-3.81" width="0" layer="20"/>
<wire x1="149.86" y1="-3.81" x2="-2.54" y2="-3.81" width="0" layer="20"/>
</plain>
<libraries>
<library name="avr-5">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="BAT-HLD-001">
</package>
<package name="2X3-NS">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="Seeed-Discrete">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="PS12">
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="FSMJSMA">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO214AC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="avr-5" package="SOIC14" value="TINY24/44/84-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS">
<attribute name="NAME"/>
</element>
<element name="Q1" library="Seeed-Discrete" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="SparkFun" package="BAT-HLD-001" value=""/>
<element name="C2" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0603-RES" value="10K"/>
<element name="D2" library="microbuilder" package="SOD-523" value="DIODE-SCHOTTKY_"/>
<element name="C4" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="R2" library="SparkFun" package="0603-RES" value="510K"/>
<element name="R3" library="SparkFun" package="0603-RES" value="100R"/>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="C5" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="SP1" library="adafruit" package="PS12" value="SPEAKER/PS12"/>
<element name="D1" library="diode" package="DO214AC" value=""/>
<element name="SW1" library="adafruit" package="FSMJSMA" value="SPST_TACTFSMJSMA"/>
<element name="IC2" library="avr-5" package="SOIC14" value="TINY24/44/84-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS">
<attribute name="NAME"/>
</element>
<element name="Q2" library="Seeed-Discrete" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B2" library="SparkFun" package="BAT-HLD-001" value=""/>
<element name="C1" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun" package="0603-RES" value="10K"/>
<element name="D3" library="microbuilder" package="SOD-523" value="DIODE-SCHOTTKY_"/>
<element name="C7" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="R11" library="SparkFun" package="0603-RES" value="510K"/>
<element name="R12" library="SparkFun" package="0603-RES" value="100R"/>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="C8" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="SP2" library="adafruit" package="PS12" value="SPEAKER/PS12"/>
<element name="D4" library="diode" package="DO214AC" value=""/>
<element name="SW2" library="adafruit" package="FSMJSMA" value="SPST_TACTFSMJSMA"/>
<element name="IC3" library="avr-5" package="SOIC14" value="TINY24/44/84-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS">
<attribute name="NAME"/>
</element>
<element name="Q3" library="Seeed-Discrete" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B3" library="SparkFun" package="BAT-HLD-001" value=""/>
<element name="C9" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun" package="0603-RES" value="10K"/>
<element name="D5" library="microbuilder" package="SOD-523" value="DIODE-SCHOTTKY_"/>
<element name="C11" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="R17" library="SparkFun" package="0603-RES" value="510K"/>
<element name="R18" library="SparkFun" package="0603-RES" value="100R"/>
<element name="LED3" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="C12" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="SP3" library="adafruit" package="PS12" value="SPEAKER/PS12"/>
<element name="D6" library="diode" package="DO214AC" value=""/>
<element name="SW3" library="adafruit" package="FSMJSMA" value="SPST_TACTFSMJSMA"/>
<element name="IC4" library="avr-5" package="SOIC14" value="TINY24/44/84-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS">
<attribute name="NAME"/>
</element>
<element name="Q4" library="Seeed-Discrete" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B4" library="SparkFun" package="BAT-HLD-001" value=""/>
<element name="C13" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="SparkFun" package="0603-RES" value="10K"/>
<element name="D7" library="microbuilder" package="SOD-523" value="DIODE-SCHOTTKY_">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SparkFun" package="0603-RES" value="510K"/>
<element name="R24" library="SparkFun" package="0603-RES" value="100R"/>
<element name="LED4" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="C16" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="SP4" library="adafruit" package="PS12" value="SPEAKER/PS12"/>
<element name="D8" library="diode" package="DO214AC" value=""/>
<element name="SW4" library="adafruit" package="FSMJSMA" value="SPST_TACTFSMJSMA"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="B1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="SP1" pad="P$1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="6"/>
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="B1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="SW1" pad="B"/>
<contactref element="SW1" pad="B'"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="5"/>
<contactref element="R7" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="SW1" pad="A'"/>
<contactref element="SW1" pad="A"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="V_CAP">
<contactref element="D2" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="SP1" pad="P$2"/>
</signal>
<signal name="BUZZER">
<contactref element="Q1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="CAPACITANCE_V">
<contactref element="IC1" pad="12"/>
<contactref element="D2" pad="K"/>
<contactref element="C4" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="CLK_OUT">
<contactref element="IC1" pad="5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="LED_A">
<contactref element="IC1" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="LED_K">
<contactref element="IC1" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$3">
</signal>
<signal name="VCC1">
<contactref element="JP2" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="B2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="SP2" pad="P$1"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="GND1">
<contactref element="IC2" pad="14"/>
<contactref element="JP2" pad="6"/>
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="B2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="SW2" pad="B"/>
<contactref element="SW2" pad="B'"/>
</signal>
<signal name="RESET1">
<contactref element="IC2" pad="4"/>
<contactref element="JP2" pad="5"/>
<contactref element="R9" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="SW2" pad="A'"/>
<contactref element="SW2" pad="A"/>
</signal>
<signal name="MOSI1">
<contactref element="JP2" pad="4"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="MISO1">
<contactref element="IC2" pad="8"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SCK1">
<contactref element="IC2" pad="9"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="V_CAP1">
<contactref element="D3" pad="A"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="3"/>
<contactref element="R8" pad="1"/>
<contactref element="SP2" pad="P$2"/>
</signal>
<signal name="BUZZER1">
<contactref element="Q2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="CAPACITANCE_V1">
<contactref element="IC2" pad="12"/>
<contactref element="D3" pad="K"/>
<contactref element="C7" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="CLK_OUT1">
<contactref element="IC2" pad="5"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="LED_A1">
<contactref element="IC2" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="LED_K1">
<contactref element="IC2" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="R12" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="VCC2">
<contactref element="JP3" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="B3" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="SP3" pad="P$1"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="GND2">
<contactref element="IC3" pad="14"/>
<contactref element="JP3" pad="6"/>
<contactref element="Q3" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="B3" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="D6" pad="A"/>
<contactref element="SW3" pad="B"/>
<contactref element="SW3" pad="B'"/>
</signal>
<signal name="RESET2">
<contactref element="IC3" pad="4"/>
<contactref element="JP3" pad="5"/>
<contactref element="R15" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="SW3" pad="A'"/>
<contactref element="SW3" pad="A"/>
</signal>
<signal name="MOSI2">
<contactref element="JP3" pad="4"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="MISO2">
<contactref element="IC3" pad="8"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="SCK2">
<contactref element="IC3" pad="9"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="V_CAP2">
<contactref element="D5" pad="A"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="Q3" pad="3"/>
<contactref element="R14" pad="1"/>
<contactref element="SP3" pad="P$2"/>
</signal>
<signal name="BUZZER2">
<contactref element="Q3" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="CAPACITANCE_V2">
<contactref element="IC3" pad="12"/>
<contactref element="D5" pad="K"/>
<contactref element="C11" pad="1"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="CLK_OUT2">
<contactref element="IC3" pad="5"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="LED_A2">
<contactref element="IC3" pad="3"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="LED_K2">
<contactref element="IC3" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="R18" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="VCC3">
<contactref element="JP4" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="B4" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="SP4" pad="P$1"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="GND3">
<contactref element="IC4" pad="14"/>
<contactref element="JP4" pad="6"/>
<contactref element="Q4" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="B4" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="D8" pad="A"/>
<contactref element="SW4" pad="B"/>
<contactref element="SW4" pad="B'"/>
</signal>
<signal name="RESET3">
<contactref element="IC4" pad="4"/>
<contactref element="JP4" pad="5"/>
<contactref element="R21" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="SW4" pad="A'"/>
<contactref element="SW4" pad="A"/>
</signal>
<signal name="MOSI3">
<contactref element="JP4" pad="4"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="MISO3">
<contactref element="IC4" pad="8"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="SCK3">
<contactref element="IC4" pad="9"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="V_CAP3">
<contactref element="D7" pad="A"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="Q4" pad="3"/>
<contactref element="R20" pad="1"/>
<contactref element="SP4" pad="P$2"/>
</signal>
<signal name="BUZZER3">
<contactref element="Q4" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="CAPACITANCE_V3">
<contactref element="IC4" pad="12"/>
<contactref element="D7" pad="K"/>
<contactref element="C15" pad="1"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="CLK_OUT3">
<contactref element="IC4" pad="5"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="LED_A3">
<contactref element="IC4" pad="3"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="LED_K3">
<contactref element="IC4" pad="2"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="R24" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
