<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="44.12" y2="0" width="0" layer="20"/>
<wire x1="44.12" y1="0" x2="44.12" y2="17.77" width="0" layer="20"/>
<wire x1="44.12" y1="17.77" x2="0" y2="17.77" width="0" layer="20"/>
<wire x1="0" y1="17.77" x2="0" y2="0" width="0" layer="20"/>
<text>T+</text>
<text>T-</text>
<text>1-Wire Thermocouple Sensor (K-Type) r3</text>
<text>6-Wire 1Wire Network</text>
<text>Yel</text>
<text>Red</text>
<text>Copyright 2015 Oregon State University</text>
<text>Trademark Sensiplicity Systems</text>
<hole x="27.305" y="3.81" drill="3.2"/>
</plain>
<libraries>
<library name="NA-lib">
<packages>
<package name="TDFN-10-4X3">
</package>
<package name="RJ-12-SHORT">
</package>
<package name="SOT753-5">
</package>
<package name="0603-CAP">
</package>
<package name="SOT23-3">
</package>
<package name="0603-RES">
</package>
<package name="TE_TERMINAL_1986711-2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="NA-lib" package="TDFN-10-4X3" value="MAX31850">
<attribute name="NAME"/>
</element>
<element name="J1" library="NA-lib" package="RJ-12-SHORT" value="PULSE_E5566-Q0LK22-L">
<attribute name="NAME"/>
</element>
<element name="U2" library="NA-lib" package="SOT753-5" value="TCR2EF33,LM">
<attribute name="NAME"/>
</element>
<element name="C1" library="NA-lib" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="NA-lib" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="NA-lib" package="SOT23-3" value="RK7002BT116">
<attribute name="NAME"/>
</element>
<element name="R1" library="NA-lib" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="NA-lib" package="0603-CAP" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="NA-lib" package="0603-RES" value=""/>
<element name="FB2" library="NA-lib" package="0603-RES" value=""/>
<element name="J2" library="NA-lib" package="TE_TERMINAL_1986711-2" value="1986711-2">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="PAD"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="9"/>
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="3V3">
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="5"/>
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="FB2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="FB1" pad="1"/>
</signal>
<signal name="T-TERM">
<contactref element="FB2" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="T+TERM">
<contactref element="J2" pad="2"/>
<contactref element="FB1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="3"/>
<contactref element="J1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
