<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="41.91" y2="0" width="0" layer="20"/>
<wire x1="41.91" y1="0" x2="41.91" y2="17.78" width="0" layer="20"/>
<wire x1="41.91" y1="17.78" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<text>ADM4850</text>
<text>TERM_EN</text>
<text>USB-RS485 Bridge</text>
</plain>
<libraries>
<library name="NA-lib">
<packages>
<package name="RJ-12-SHORT">
</package>
<package name="LSCSP-8">
</package>
<package name="USB_B_CONNECTOR_TH">
</package>
<package name="SSOP-28">
</package>
<package name="0603-CAP-POL">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="NA-lib" package="RJ-12-SHORT" value="PULSE_E5566-Q0LK22-L">
<attribute name="NAME"/>
</element>
<element name="U2" library="NA-lib" package="LSCSP-8" value="ADM4850ACPZ">
<attribute name="NAME"/>
</element>
<element name="J2" library="NA-lib" package="USB_B_CONNECTOR_TH" value="USB-B1HSW6">
<attribute name="NAME"/>
</element>
<element name="U1" library="NA-lib" package="SSOP-28" value="FT232RL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="NA-lib" package="0603-CAP-POL" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="NA-lib" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="1206" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="J2" pad="5V"/>
<contactref element="C1" pad="+"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="20"/>
<contactref element="U2" pad="8"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="GND"/>
<contactref element="J2" pad="SHIELD_1"/>
<contactref element="J2" pad="SHIELD_2"/>
<contactref element="C1" pad="-"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="26"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="PAD"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="D+"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="D-"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="17"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="6"/>
<contactref element="J1" pad="4"/>
<contactref element="J3" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="7"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="J3" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
