<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="30.48" width="0" layer="20"/>
<wire x1="35.56" y1="30.48" x2="0" y2="30.48" width="0" layer="20"/>
<wire x1="0" y1="30.48" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="3.81" drill="3.175"/>
<text>Always-On
LED</text>
<text>Response
LED</text>
<text>Help
Switch</text>
<hole x="3.81" y="26.67" drill="3.175"/>
<text>Emergency Button r2
Copyright 2015 
Oregon State University
Trademark Sensiplicity Systems</text>
</plain>
<libraries>
<library name="NA-lib">
<packages>
<package name="RJ-12-SHORT">
</package>
<package name="TSOC-6">
</package>
<package name="HEADER-02">
</package>
<package name="0603-RES">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="NA-lib" package="RJ-12-SHORT" value="E5566-Q0LK22-L">
<attribute name="NAME"/>
</element>
<element name="U1" library="NA-lib" package="TSOC-6" value="DS2413">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="NA-lib" package="HEADER-02" value=""/>
<element name="R2" library="NA-lib" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="NA-lib" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="NA-lib" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="NA-lib" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="NA-lib" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="NA-lib" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="SW1" pad="2"/>
<contactref element="LED2" pad="K"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="1WIRE">
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="6"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="SW1" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
